For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Move the window to the full up position.

1 | Front Side Door Check Link Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Check Link Nut (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Front Side Door Check Link Assembly Tip Remove the check link from the inside of the door.