For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear end trim finish panel. Refer to Rear End Trim Finish Panel Replacement.

1 | Rear Compartment Lift Window Latch Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
10 N·m (89 lb in)

2 | Rear Compartment Lift Window Latch