For 1990-2009 cars

#### Tools Required

J 45059 Angle Meter

Important: Do not use any sealing material.

1. Install the cylinder head gasket to the block.
2. Install the cylinder head.

Notice: Refer to Fastener Notice in the Preface section.

Important: Always use new cylinder head bolts.

3. Install and tighten the cylinder head bolts in sequence.

Tighten

• | Tighten the bolts to 30 N·m (22 lb ft).

• | Tighten the bolts an additional 155 degrees in sequence. Use the J 45059 .

4. Install the front cylinder head bolts.

Tighten
Tighten the cylinder head bolts to 35 N·m (26 lb ft).