For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Trunk Release Relay B+ | 1 | 1 | -- | --
Rear Compartment Lid Release Switch Signal | 2 | 2 | 2 | --
Folding Top Cover Actuator Control | 1 | 1 | 1 | --
Trunk Release Relay Control | B3265 06 | B3265 06 | B3265 01 | --
Rear Compartment Lid Release Actuator Control | 2 | 2 | 2 | --
Folding Top Cover Actuator Ground | -- | 1 | -- | --
Rear Compartment Lid Release Actuator Ground | -- | 1 | -- | --
Rear Compartment Lid Release Switch Ground | -- | 2 | -- | --
1. Rear Compartment Lid Release Malfunction 2. Rear Compartment Lid Release Switch Malfunction

### Circuit/System Description

When the rear compartment lid release switch is operated, the rear compartment lid release switch signal circuit to the body control module (BCM) is switched to ground. The BCM receives the rear compartment lid release switch input and applies ground to the rear compartment lid relay control circuit. This energizes the trunk release relay coil, closing the switch side contacts, allowing battery voltage to be applied to the rear compartment lid release actuator and folding top cover actuator, releasing the folding top cover and opening the rear compartment lid.

### Reference Information

#### Schematic Reference

Release Systems Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Luggage Compartment Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. Ignition ON, observe the scan tool Trunk Release Switch parameter while pressing the rear compartment lid release switch. The parameter should change between Active and Inactive.

⇒ | If the value does not change as the switch is pressed, refer to Rear Compartment Lid Release Switch Malfunction.

2. Command the Trunk Release with a scan tool. The folding top cover actuator and rear compartment lid release actuator should release the folding top cover and the rear compartment lid.

⇒ | If the folding top cover or rear compartment lid does not release, refer to Rear Compartment Lid Release Malfunction.

### Circuit/System Testing

#### Rear Compartment Lid Release Switch Malfunction

1. Ignition OFF, disconnect the harness connector at the rear compartment lid release switch.
2. Verify that a test lamp illuminates between B+ and the ground circuit terminal A.

⇒ | If the test lamp does not illuminate, test the ground circuit for an open/high resistance.

3. Ignition ON, verify the scan tool Trunk Release Switch parameter is Inactive.

⇒ | If not the specified value, test the signal circuit terminal C for a short to ground. If circuit tests normal, replace the BCM.

4. Install a 3A fused jumper wire between the signal circuit terminal C and ground. Verify the scan tool Trunk Release Switch parameter is Active.

⇒ | If not the specified value, test the signal circuit for a short to voltage or an open/high resistance. If circuit tests normal, replace the BCM.

5. If all circuits test normal, test or replace the rear compartment lid release switch.

#### Rear Compartment Lid Release Malfunction

1. Ignition OFF, disconnect the TRUNK RELSE relay.
2. Ignition ON, verify that a test lamp does not illuminate between the control circuit terminal 87 and ground.

⇒ | If the test lamp illuminates, test the control circuit for a short to voltage.

3. Verify that a test lamp illuminates between the B+ circuit terminal 85 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for an open/high resistance. If the circuit tests normal and the B+ circuit fuse is open, test the control circuit terminal 86 for a short to ground. If the circuit tests normal, test or replace the TRUNK RELSE relay.

4. Verify that a test lamp illuminates between the B+ circuit terminal 30 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance. If the circuit tests normal and the B+ circuit fuse is open, test the control circuit terminal 87 for a short to ground.

5. Ignition OFF, disconnect the harness connector at the folding top cover actuator.
6. Test for less than 5 ohms between the ground circuit terminal B and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

7. Connect the harness connector at the folding top cover actuator.
8. Ignition ON, connect a 25A fused jumper wire between the B+ circuit terminal 30 and the control circuit terminal 87. Verify the folding top cover actuator is activated.

⇒ | If the folding top cover actuator does not activate, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, test or replace the folding top cover actuator.

9. Ignition OFF, disconnect the harness connector at the rear compartment lid release actuator.
10. Test for less than 5 ohms between the ground circuit terminal B and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

11. Connect the harness connector at the rear compartment lid release actuator.
12. Ignition ON, connect a 25A fused jumper wire between the B+ circuit terminal 30 and the control circuit terminal 87. Verify the rear compartment lid release actuator is activated.

⇒ | If the rear compartment lid release actuator does not activate, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, test or replace the rear compartment lid release actuator.

13. Connect a test lamp between the B+ circuit terminal 85 and the control circuit terminal 86.
14. Command the Trunk Release with a scan tool with a scan tool. The test lamp should illuminate when commanding the rear compartment lid release actuator.

⇒ | If the test lamp is always ON, test the control circuit for a short to ground. If the circuit tests normal, replace the BCM.

⇒ | If the test lamp is always OFF, test the control circuit for a short to voltage or an open/high resistance. If the circuit tests normal, replace the BCM.

15. If all circuits test normal, test or replace the TRUNK RELSE relay.

### Component Testing

#### Rear Compartment Lid Release Switch

1. Ignition OFF, disconnect the harness connector at the rear compartment lid release switch.
2. Test for infinite resistance between the ground terminal A and the signal terminal C with the switch in the open position.

⇒ | If not the specified value, replace the rear compartment lid release switch.

3. Test for less than 2 ohms between the ground terminal A and the signal terminal C with the switch in the closed position.

⇒ | If greater than the specified range, replace the rear compartment lid release switch.

#### Trunk Release Relay

1. Ignition OFF, disconnect the TRUNK RELSE relay.
2. Test for 60-200 ohms between terminals 85 and 86.

⇒ | If not within the specified range, replace the relay.

3. Test for infinite resistance between the following terminals:

• | 30 and 86

• | 30 and 87

• | 30 and 85

• | 85 and 87

⇒ | If less than the specified value, replace the relay.

4. Install a 3A fused jumper wire between relay terminal 85 and 12V. Install a jumper wire between relay terminal 86 and ground. Test for less than 2 ohms between terminals 30 and 87.

⇒ | If greater than specified range, replace the relay.

#### Rear Compartment Lid Release Actuator

1. Ignition OFF, disconnect the harness connector at the rear compartment lid release actuator.
2. Install a 25A fused jumper between the control terminal A and 12V. Install a jumper between the ground terminal B and ground. Verify the actuator activates.

⇒ | If the actuator does not activate, replace the rear compartment lid release actuator.

#### Folding Top Cover Actuator

1. Ignition OFF, disconnect the harness connector at the folding top cover actuator.
2. Install a 25A fused jumper between the control terminal A and 12V. Install a jumper between the ground terminal B and ground. Verify the actuator activates.

⇒ | If the actuator does not activate, replace the folding top cover actuator.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Rear Compartment Lid Latch Replacement

• | Rear Compartment Lid Release Switch Replacement

• | Relay Replacement

• | Rear Compartment Lid Buttress Latch Release Cable Replacement

• | Control Module References for BCM replacement, setup and programming