For 1990-2009 cars

### Removal Procedure

1. Remove the starter. Refer to Starter Motor Replacement .
2. Disconnect the crankshaft position (CKP) sensor electrical connector (1).
3. Remove the CKP sensor bolt.
4. Remove the CKP sensor.

### Installation Procedure

1. Lubricate the CKP sensor O-ring seal with clean engine oil.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CKP sensor.
3. Install the CKP sensor bolt.

Tighten
Tighten the sensor bolt to 10 N·m (89 lb in).

4. Connect the CKP sensor electrical connector (1).
5. Install the starter. Refer to Starter Motor Replacement .