For 1990-2009 cars

## Windshield Washer Solvent Container Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
2. Drain the washer solvent into a suitable clean container.

1 | Windshield Washer Pump Hose Assembly

#### Procedure

1. Disconnect the hose at the hinge pillar and air inlet panel.
2. Disengage the integral washer hose clip from the electronic control module (ECM) bracket.

2 | Windshield Washer Solvent Container Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
3 | Windshield Washer Container Assembly Tip Lower the windshield washer container from behind the left front fender area.
4 | Windshield Washer Container Pump Kit Tip Disconnect the washer hose at the pump and use 2 flat-bladed tools and pry the washer pump from the container.

## Windshield Washer Solvent Container Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
2. Drain the washer solvent into a suitable clean container.

1 | Windshield Washer Pump Hose Assembly

#### Procedure

1. Disconnect the hose at the hinge pillar and air inlet panel.
2. Disengage the integral washer hose clip from the electronic control module (ECM) bracket.

2 | Windshield Washer Solvent Container Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
3 | Windshield Washer Container Assembly Tip Lower the windshield washer container from behind the left front fender area.
4 | Windshield Washer Container Pump Kit Tip Disconnect the washer hose at the pump and use 2 flat-bladed tools and pry the washer pump from the container.