For 1990-2009 cars

## Radio Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement .
2. Program the radio after replacement. Refer to Control Module References .

1 | Radio Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | AM/FM Stereo Radio Assembly

## Radio Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Program the radio after replacement. Refer to Control Module References .

1 | Radio Bolt/Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | AM/FM Stereo Radio