For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement .

1 | Evaporator Case Seal
2 | Thermal Expansion Valve Bolt (Qty: 2) Tighten 16 N·m (12 lb ft)
3 | Thermal Expansion Valve
4 | Sealing Washer Tip Remove and discard seals. Refer to Sealing Washer Replacement .
5 | Rear Air Outlet Duct Screw (Qty: 2) Tighten 1.5 N·m (13 lb in)
6 | Rear Air Outlet Duct
7 | Evaporator Case Assembly Screw (Qty: 9) Tighten 1.5 N·m (13 lb in)
8 | Evaporator Lower Case
9 | Evaporator Core