For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate capacities are given in English and metric conversions. Please refer to Recommended Fluids and Lubricants for more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant R134a | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer/retailer for more information.
Cooling System

- 2.0L L4 Engine -- Automatic

9.2 qt

8.7 L

- 2.0L L4 Engine -- Manual

9.5 qt

9.0 L

- 2.4L L4 Engine -- Automatic

8.7 qt

8.2 L

- 2.4L L4 Engine -- Manual

8.9 qt

8.4 L

Engine Oil with Filter

- 2.0L L4 and 2.4L L4

5.0 qt

4.7 L

Fuel Tank | 13.6 gal | 51.5 L
Transmission, Automatic (Bottom Pan Removal) | 7.4 qt | 7.0 L
Transmission, Manual (Complete Drain and Refill) | 2.75 qt | 2.6 L
Wheel Nut Torque | 100 lb ft | 140 N·m
All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual.

#### Engine Specifications

Engine | VIN Code | Transmission | Spark Plug Gap
--- | --- | --- | ---
2.0L L4 | X | Automatic Manual | 0.035 in (0.9mm)
2.4L L4 | B | Automatic Manual | 0.040 in (1.01 mm)