For 1990-2009 cars

### Removal Procedure

1. Loosen the charge air cooler hose clamp (1) at the throttle body.
2. Loosen the charge air cooler hose clamp (2) at the charge air cooler outlet pipe.
3. Remove the charge air cooler hose from the throttle body and the outlet pipe.

### Installation Procedure

1. Install the charge air cooler hose to the outlet pipe and the throttle body.
2. Tighten the charge air cooler hose clamp (2) at the charge air cooler outlet pipe.

Caution: Refer to Fastener Caution in the Preface section.

3. Tighten the charge air cooler hose clamp (1) at the throttle body.

Tighten
Tighten the charge air cooler hose clamps to 5 N·m (44 lb in).