For 1990-2009 cars

## Evaporative Emission Canister Replacement Convertible

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement.
2. Remove the evaporative emission (EVAP) canister/fuel tank line. Refer to Evaporative Emission Hoses/Pipes Replacement - Canister/Fuel Tank.
3. Slide the EVAP canister upward from the bracket.

### Installation Procedure

1. Slide the NEW EVAP canister down into the bracket.
2. Install the EVAP canister/fuel tank line. Refer to Evaporative Emission Hoses/Pipes Replacement - Canister/Fuel Tank.
3. Install the fuel tank. Refer to Fuel Tank Replacement.