For 1990-2009 cars

## Digital Radio Antenna Replacement Convertible

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | Bolt, Mobile Telephone and Vehicle Location Antenna Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Expansion Sleeve, Mobile Telephone and Vehicle Location Antenna
3 | Antenna and Base Assembly, Mobile Telephone and Vehicle Location

## Digital Radio Antenna Replacement Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lower the Headlining Rear Trim Panel to access the antenna base fastener. Refer to Headlining Rear Trim Panel Replacement

1 | Digital Radio Antenna Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Loosen the integral bolt.
2. Disconnect the electrical connections.
3. Disconnect the antenna cables.
4. Feed the wiring and cable up through the hole in the roof panel.

Tighten
10 N·m (89 lb in)