For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Roof Lift Off Panel Weatherstrip Fastener (Qty:4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Place the roof panel on a protective surface.

Tighten
Tighten the weatherstrip fastener to 2 N·m (89 bl in).

2 | Roof Lift Off Panel Weatherstrip

#### Procedure

1. Using a 50/50 mix of soap and water (lubricant ) on the back side of the weatherstrip this will aid in the reinstalling the weatherstrip to the retainer. Push firmly on the front and rear ends of the weatherstrip to ensure that the bead is secured to the frame.
2. Ensure proper alignment for the window and roof lift off panel to prevent water leaks. Refer to Roof Lift Off Panel Adjustment.