For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the power steering pump drive belt. Refer to Power Steering Pump Belt Replacement .

1 | Power Steering Pump Pulley

#### Procedure

1. Use the remover J 25034-C (for Pontiac) or remover SA9162C-2 (for Saturn) to remove the power steering pump pulley.
2. Use installer J 25033-C (for Pontiac) or replacer SA9162C-2 (for Saturn) to install the power steering pump pulley.
3. Ensure the axial tolerance of the power steering pulley on the power steering pump is within 0.25 mm (0.010 in).

#### Special Tools

• | J 25033-C Pulley Installer

• | J 25034-C Pulley Remover

• | SA9162C-2 Power Steering Pump Pulley Remover/Replacer