For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the panel. Refer to Front Floor Panel Carpet Filler Replacement .
2. Program the body control module after replacement. Refer to Control Module References .

1 | Body Control Module Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tip Disconnect the electrical connectors. Tighten
2.5 N·m (53 lb in)

2 | Body Control Module Assembly