For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Remove the instrument panel (I/P) cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Disconnect the electrical connectors.

1 | Screw, Control Assembly - Heater and Air Conditioning (Qty: 4) Tighten 1.5 N·m (13 lb in)
2 | Control Assembly, Heater and Air Conditioning