For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Disconnect the ignition coil electrical connector(s).
3. Remove the ignition coil bolt(s).
4. Remove the ignition coil(s).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the ignition coil(s).
2. Install the ignition coil bolt(s).

Tighten
Tighten the bolt(s) to 10 N·m (89 lb in).

3. Connect the ignition coil electrical connector(s).
4. Install the intake manifold cover. Refer to Intake Manifold Cover Replacement .