For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) carrier. Refer to Instrument Panel Carrier Replacement .

1 | Heater Core Cover Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Heater Core Cover
3 | Air Conditioning Refrigerant Temperature Sensor Tip

1. Disconnect the air conditioning refrigerant temperature sensor electrical connector.
2. Twist the air conditioning refrigerant temperature sensor to the left to release and pull upward.