For 1990-2009 cars

### Removal Procedure

1. Remove the left engine mount. Refer to Engine Mount Replacement - Left Side .
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the starter solenoid positive battery cable nut (4) from the starter.
4. Remove the positive battery cable terminal (5) from the starter.
5. Reposition the positive battery cable boot (4).
6. Remove the generator positive battery cable nut (2) from the generator.
7. Remove the positive battery cable terminal (5) from the generator.
8. Remove the engine harness clip (4) from the intake manifold.
9. Remove the left side engine mount bracket bolts and bracket.

### Installation Procedure

1. Position the left engine mount bracket to the engine block.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the left engine mount bracket bolts until snug.
3. Tighten the left engine mount bracket bolts.

Tighten
Tighten the bolts in the sequence shown to 55 N·m (41 lb ft).

4. Install the positive battery cable terminal (5) to the generator.
5. Install the generator positive battery cable nut (2) to the generator.

Tighten
Tighten the nut to 20 N·m (15 lb ft).

6. Position the positive battery cable boot (4).
7. Install the engine harness clip (4) to the intake manifold.
8. Install the positive battery cable terminal (5) to the starter.
9. Install the starter solenoid positive battery cable nut (4) to the starter.

Tighten
Tighten the nut to 10 N·m (89 lb in).

10. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation .
11. Install the left engine mount. Refer to Engine Mount Replacement - Left Side .