For 1990-2009 cars

Name | 5L40
--- | ---
RPO Codes | M82
Production Location | Strasbourg, France
Vehicle Platform Engine/Transmission Usage | M
Transmission Drive | Rear Wheel Drive
1st Gear Ratio | 3.42:1
2nd Gear Ratio | 2.21:1
3rd Gear Ratio | 1.60:1
4th Gear Ratio | 1.00:1
5th Gear Ratio | 0.75:1
Reverse Ratio | 3.03:1
Torque Converter Size - Diameter of Torque Converter Turbine | 245 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | DEXRON™ VI
Transmission Fluid Capacity - Approximate | Bottom Pan Removal Complete Overhaul: Dry 8.9L (9.4 qt)
Transmission Type: 5 | Five Forward Gears
Transmission Type: L | Longitude Mount
Transmission Type: 40 | Product Series
Transmission Type: E | Electronic Controls
Position Quadrant | P, R, N, D, 4, 3, 2
Case Material | Die Cast Aluminum
Transmission Weight Dry | 73 kg (161 lb)
Transmission Net Weight | 80.5 kg (161 lb)
Maximum Trailer Towing Capacity | Domestic: 454 kg Export: 1,815 kg
Maximum Gross Vehicle Weight | 3 500 kg (7,716 lb)