For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Important: Position the surge tank to the side leaving the cooling system closed.

Remove the surge tank. Refer to Radiator Surge Tank Replacement .

1 | Radiator Surge Tank Bracket Nut (Qty: 2) Tighten 9 N·m (80 lb in)
2 | Radiator Surge Tank Support Bracket