For 1990-2009 cars

## Transmission Support Replacement Manual Transmission

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front floor closeout panel. Refer to Floor Panel Tunnel Panel Replacement - Front .
3. Remove the floor panel tunnel rear panel. Refer to Floor Panel Tunnel Panel Replacement - Rear .
4. Support the transmission.

1 | Transmission Support Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 58 N·m (43 lb ft)
2 | Transmission Support

## Transmission Support Replacement Automatic Transmission

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front floor closeout panel. Refer to Floor Panel Tunnel Panel Replacement - Front .
3. Remove the floor panel tunnel rear panel. Refer to Floor Panel Tunnel Panel Replacement - Rear .
4. Support the transmission.

1 | Transmission Mount Nut (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Transmission Support Bolt (Qty: 4) Tighten 58 N·m (43 lb ft)
3 | Transmission Support