For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Refrigerant Valve | 11 N·m | 98 lb in
Bolt, A/C Compressor | 22 N·m | 16 lb ft
Bolt, A/C Condenser | 9 N·m | 80 lb in
Bolt, Distributor Air | 2.5 N·m | 16 lb in
Bolt, Hose Assembly, A/C Compressor and Condenser Hose | 22 N·m | 16 lb ft
Bolt, Radiator Assembly | 25 N·m | 18 lb ft
Bolt, Receiver Dehydrator Assembly | 6 N·m | 53 lb in
Bolt, Thermal Expansion Valve | 16 N·m | 12 lb ft
Bolt, Thermal Expansion Valve | 1.5 N·m | 13 lb in
Nut, A/C Condenser Tube | 9 N·m | 80 lb in
Nut, Air Inlet Housing | 9 N·m | 80 lb in
Nut, Distributor Air | 2.5 N·m | 16 lb in
Nut, Hose Assembly, A/C Compressor and Condenser Hose | 9 N·m | 80 lb in
Nut, Hose Assembly, A/C Evaporator | 16 N·m | 12 lb ft
Nut, Hose Assembly, A/C Evaporator Clip | 9 N·m | 80 lb in
Nut, HVAC Module Assembly | 9 N·m | 80 lb in
Nut, Tube Assembly, A/C Compressor | 16 N·m | 12 lb ft
Nut, Tube Assembly, A/C Condenser | 9 N·m | 80 lb in
Screw, Air Distribution Case | 1.5 N·m | 13 lb in
Screw, Air Inlet Housing | 1.5 N·m | 13 lb in
Screw, Air Outlet Duct | 1.5 N·m | 13 lb in
Screw, Blower Motor | 1.5 N·m | 13 lb in
Screw, Blower Motor Resistor | 1.5 N·m | 13 lb in
Screw, Evaporator Case Assembly | 1.5 N·m | 13 lb in
Screw, Heater Core Cover | 1.5 N·m | 13 lb in
Screw, Mode Actuator | 1.5 N·m | 13 lb in
Screw, Rear Air Outlet Duct | 1.5 N·m | 13 lb in
Screw, Receiver Dehydrator | 1.5 N·m | 13 lb in
Sensor, A/C Refrigerant Pressure | 5 N·m | 44 lb in