For 1990-2009 cars

## Windshield Wiper Transmission Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .
3. Disengage the connector positive assurance (CPA) clip from the wiper motor electrical connector.
4. Disconnect the wiper motor electrical connector from the wiper motor.

1 | Windshield Washer System Module Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Install the driver side bolt first.
2. Install the passenger side bolt second.
3. Install the center bolt third.

Tighten
9 N·m (80 lb in)

2 | Windshield Washer System Module Assembly

## Windshield Wiper Transmission Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .
3. Disengage the connector positive assurance (CPA) clip from the wiper motor electrical connector.
4. Disconnect the wiper motor electrical connector from the wiper motor.

1 | Windshield Washer System Module Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Tighten the bolts in sequence as noted in the graphic.

Tighten
9 N·m (80 lb in)

2 | Windshield Washer System Module Bolt
3 | Windshield Washer System Module Bolt
4 | Windshield Washer System Module Assembly