For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Fluid Irritant Caution in the Preface section. Caution: Refer to Brake Dust Caution in the Preface section. Important: New brake calipers are packaged filled with brake fluid. DO NOT drain the brake fluid from the new caliper prior to installation. Draining the brake fluid from the new brake caliper will prevent the brake caliper from bleeding properly.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Release the tension from the park brake cables. Refer to Park Brake Adjustment .
4. Disconnect the park brake cable from the actuator lever on the brake caliper.

1 | Brake Hose Fitting Bolt Notice: Refer to Fastener Notice in the Preface section. Tip If installing a new brake caliper, hand install the brake hose fitting bolt, the new gaskets and the hose to the new caliper with the caliper inverted to prevent brake fluid loss.

Tighten
40 N·m (20 lb ft)

2 | Brake Hose Fitting Gasket (Qty: 2) Tip DO NOT reuse the brake hose fitting gaskets. Install NEW gaskets.
3 | Brake Hose Tip

• | Plug the brake caliper inlet port to prevent brake fluid loss and contamination.

• | Plug the brake hose fitting to prevent brake fluid loss and contamination.

4 | Brake Caliper Guide Pin Seal (Qty: 2)
5 | Brake Caliper Guide Pin (Qty: 2) Tighten 27 N·m (20 lb ft)
6 | Brake Caliper Guide Pin Bushing (Qty: 2)
7 | Brake Caliper Notice: When using a large C-clamp to compress a caliper piston into a caliper bore of a caliper equipped with an integral park brake mechanism, do not exceed more than 1 mm (0.039 in) of piston travel. Exceeding this amount of piston travel will cause damage to the internal adjusting mechanism and/or the integral park brake mechanism.

#### Procedure

1. Use a large C-clamp to compress the brake caliper piston slightly to ease caliper removal. DO NOT exceed 1 mm (0.039 in) of caliper piston travel.
2. Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .
3. With the engine OFF, gradually apply the brake pedal to approximately 2/3 of its travel distance.
4. Slowly release the brake pedal.
5. Wait 15 seconds, then repeat steps 3-4 until a firm brake pedal is obtained. This will properly seat the brake caliper piston and brake pads.
6. Fill the master cylinder reservoir. Refer to Master Cylinder Reservoir Filling .
7. Connect the park brake cable to the actuator lever on the caliper.
8. Adjust the tension of the park brake cables. Refer to Park Brake Adjustment .
9. Burnish the brake pads and rotors. Refer to Brake Pad and Rotor Burnishing .