For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front floor closeout panel. Refer to Floor Panel Tunnel Panel Replacement - Front.
3. Disconnect the vehicle speed sensor (VSS) electrical connector (2).
4. Remove the VSS bolt (1).
5. Remove the VSS (2).
6. Remove the O-ring seal (3) from the VSS (2).

### Installation Procedure

1. Install the O-ring seal (3) to the VSS (2).
2. Install the VSS (2) to the transmission.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the VSS bolt (1).

Tighten
Tighten the bolt to 17 N·m (13 lb ft).

4. Connect the VSS electrical connector (2).
5. Install the front floor closeout panel. Refer to Floor Panel Tunnel Panel Replacement - Front.
6. Lower the vehicle.