For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transmission. Refer to Transmission Replacement.
3. Remove the clutch hose from the actuator cylinder. Refer to Hydraulic Clutch Hose/Pipe Replacement.

1 | Clutch Actuator Cylinder Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use LOCTITE 592® P/N 21485278 thread sealant on the screws.

Tighten
10 N·m (89 lb in)

2 | Clutch Actuator Cylinder