For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Important: Drain only the fluid from the radiator surge tank.

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Disconnect the surge tank sensor electrical connector.

1 | Cap Assembly, Radiator Surge Tank
2 | Retainer, Radiator Surge Tank
3 | Nut, Radiator Surge Tank Tighten 9 N·m (80 lb in)
4 | Tank Assembly, Radiator Surge Tip Using J 38185 position radiator surge tank hose clamps aside and remove hoses from the radiator surge tank.