For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Open and support the hood.
2. Reach in between the bumper and front hood opening to disconnect the daytime running, park and turn signal lamp socket from the lamp housing.

1 | Daytime Running, Park and Turn Signal Lamp Socket Tip Squeeze the locking tab and rotate the bulb socket counter-clockwise from the lamp housing in order to remove.
2 | Daytime Running, Park and Turn Signal Lamp Bulb