For 1990-2009 cars

# Service Update for Inventory Vehicles Only-Exhaust Camshaft-Expires February 28, 2007

Subject: | 07026 -- Service Update for Inventory Vehicles Only - Exhaust Camshaft - Expires February 28, 2007

Models: | 2007 Pontiac Solstice GXP

| 2007 Saturn Sky Red Line

| Equipped with 2.0L (RPO LNF - VIN X) Engine

THIS SERVICE UPDATE INVOLVES VEHICLES IN DEALER/RETAILER INVENTORY ONLY AND WILL EXPIRE FEBRUARY 28, 2007.

### Purpose

This bulletin provides a service procedure to inspect and, if necessary, replace the exhaust camshaft on certain 2007 Pontiac Solstice GXP and Saturn Sky Red Line vehicles equipped with a 2.0L (RPO LNF -VIN X) engine. The exhaust camshaft in certain 2.0L engines may not meet the minimum hardness specification, which could result in premature wear, resulting in engine performance or misfire complaints.

This service procedure should be completed on involved vehicles currently in dealership/retailer inventory as soon as possible, but no later than February 28, 2007 , at which time this bulletin will expire.

### Vehicles Involved

A list of involved vehicles currently in dealer/retailer inventory is included in this bulletin and in the Administrative Message used to release this bulletin.

#### Pontiac Solstice GXP

BAC | VIN
--- | ---
115895 | 1G2MG35X17Y123598
115928 | 1G2MG35X17Y123603
163372 | 1G2MG35X17Y123553
165940 | 1G2MG35X87Y123601

#### Saturn Sky Red Line

BAC | VIN
--- | ---
223296 | 1G8MG35X97Y123578

Important: Dealers/retailers are to confirm vehicle eligibility prior to beginning repairs by using the system(s) below.

-- GM dealers should use GMVIS.

-- US Saturn retailers should use the AS/400 system.

### Parts Information - GM

Parts required to complete this service update are to be obtained from General Motors Service and Parts Operations (GMSPO). Please refer to your "involved vehicles listing" before ordering parts. Normal orders should be placed on a DRO = Daily Replenishment Order. In an emergency situation, parts should be ordered on a CSO = Customer Special Order.

Part Number | Description | Qty/ Vehicle
--- | --- | ---
12589340 | Camshaft, Exhaust | 1 (if required)
11588712 | Bolt, Camshaft Sprocket | 1 (if required)

### Parts Information - Saturn US Only

Parts required to complete this service update by involved Saturn US retailers are to be obtained from Saturn Service Parts Operations (SSPO).

Part Number | Description | Qty/ Vehicle
--- | --- | ---
12589340 | Camshaft, Exhaust | 1 (if required)
11588712 | Bolt, Camshaft Sprocket | 1 (if required)

### Service Procedure

1. Open hood.
2. Inspect Cylinder Head Assembly date code.

• | If date code is 346 or lower, no additional inspection or repairs are needed.

• | If date code is 347 or greater, proceed to step 3 to remove the cam cover and inspect exhaust cam shaft date code.

Important: The Camshaft Cover Gasket is re-useable. Inspect for any cuts or damage to the sealing surface of the gasket prior to re-using the gasket.

3. Remove the engine Camshaft Cover Assembly. Refer to Camshaft Cover Replacement 2.0L in SI for removal and installation instructions.

Important: Use a mirror to read the Camshaft code if it is difficult to see. In some cases, it may be necessary to rotate the Camshaft to see the code. If this is needed, rotate the crankshaft by hand to bring the Camshaft code into view.

4. Inspect Exhaust Camshaft code.

• | If the Exhaust Camshaft has any code other than 6M 06, M6 15 or M6 21 , no further inspection or repair is needed. Re-install the Camshaft Cover Assembly following the service procedures in SI.

• | If the Exhaust Camshaft has a code of 6M 06, M6 15 or 6M 21 , the Exhaust Camshaft needs to be replaced. Proceed to Step 5.

5. Replace the Exhaust Camshaft Assembly. Refer to Exhaust Camshaft and Lifter Replacement 2.0L in SI for removal and installation instructions.

### Claim Information - GM

For vehicles repaired under this service update, use:

Labor Operation | Description | Labor Time
--- | --- | ---
Y0137 | Inspect cylinder head date code. | 0.2
Remove cam cover and inspect exhaust camshaft date code. | Add: 0.7
Replace exhaust camshaft. | Add: 1.5

### Claim Information - US Saturn

To receive credit, submit a claim with the information below:

Labor Operation | Description | Case Type | Labor Time
--- | --- | --- | ---
Y0137 | Inspect cylinder head date code. | VW | 0.2
Remove cam cover and inspect exhaust camshaft date code. | Add: 0.7
Replace exhaust camshaft. | Add: 1.5