For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the intake manifold studs in the manifold face.

Tighten
Tighten the intake manifold studs to 6 N·m (53 lb in).

2. Install a new intake manifold gasket on the intake manifold.
3. Install the intake manifold.
4. Install the intake manifold bolts and nuts.

Tighten
Tighten the bolts and nuts to 10 N·m (89 lb in).

5. Lubricate the fuel injector tip insulators with engine oil.
6. Install new fuel injector tip insulators.
7. Lubricate the fuel injector oil rings with engine oil.
8. Install the fuel rail assembly.
9. Install the fuel rail bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

10. Install a new throttle body gasket.
11. Install the throttle body.

Tighten
Tighten the bolts and nuts to 10 N·m (89 lb in).

Important: Ensure that the rear metal tab of the EVAP emission canister valve is resting on the power steering pump metal body.

12. Install the EVAP emission canister valve (2).

Tighten
Tighten the EVAP canister valve bolt to 22 N·m (16 lb ft).

13. Install the EVAP emission canister valve tube (1).