For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the power steering pump drive belt. Refer to Power Steering Pump Belt Replacement .

1 | Power Steering Pump Pulley

#### Procedure

1. Using the SA9162C-2 remove the power steering pump pulley.
2. Using the SA9162C install the power steering pump pulley.
3. Ensure the axial tolerance of the power steering pulley on the power steering pump is within 0.25 mm (0.010 in).

#### Special Tools

• | SA9162C Power Steering Pump Pulley Remover/Replacer

• | SA9162C-2 Pulley Replacer