For 1990-2009 cars

## Headlamp Bulb Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open and support the hood.

1 | Side Marker Lamp Bulb Tip Twist the lamp socket counterclockwise and pull the bulb straight out from the socket.
2 | Headlamp Bulb - Lo Beam Tip Disconnect the electrical connector prior to removing the bulb.
3 | Headlamp Bulb - Hi Beam Tip Disconnect the electrical connector prior to removing the bulb.
4 | Headlamp Bulb Accessory Cover (Qty: 2) Tip Turn the accessory bulb covers a quarter turn counterclockwise and remove.

## Headlamp Bulb Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Lift upward on the connector position assurance (CPA) to release the electrical harness from the bulb socket.
3. Disconnect the electrical connector.

1 | Headlamp Bulb Socket Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Turn the bulb socket counterclockwise in order to remove.