For 1990-2009 cars

## Drive Belt Replacement With A/C

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Remove the power steering pump drive belt. Refer to Power Steering Pump Belt Replacement .
3. Lower the vehicle.
4. Remove the air cleaner. Refer to Air Cleaner Assembly Replacement .

1 | Belt, Accessory Drive

## Drive Belt Replacement Without A/C

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Remove the power steering pump drive belt. Refer to Power Steering Pump Belt Replacement .
3. Lower the vehicle.
4. Remove the air cleaner. Refer to Air Cleaner Assembly Replacement .

1 | Belt, Accessory Drive