For 1990-2009 cars

## Front Bumper Fascia Replacement SKY Base

Callout | Component Name
--- | ---
1 | Front Fascia Retainer (Qty: 16)
2 | Front Fascia Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Fascia Bracket Screw (Qty: 4) Tighten 2 N·m (18 lb in)
4 | Front Fascia Center Bracket Retainer
5 | Front Fascia Tip Disconnect the lamp connectors.

## Front Bumper Fascia Replacement SKY Turbo

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the brake cooling duct retainer. Refer to Front Brake Caliper Cooling Duct Replacement .

1 | Front Fascia Retainer (Qty: 16)
2 | Front Fascia Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Fascia Bracket Screw (Qty: 4) Tighten 2 N·m (18 lb in)
4 | Front Fascia Center Bracket Retainer
5 | Front Fascia Tip Disconnect the lamp connectors.

## Front Bumper Fascia Replacement Solstice Base

Callout | Component Name
--- | ---
1 | Front Fascia Retainers (Qty: 5)
2 | Front Fascia Retainers (Qty: 10)
3 | Wheelhouse Liner Screws (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
4 | Front Fascia Bolts (Qty: 2) Tighten 10 N·m (89 lb in)
5 | Front Fascia Bolts (Qty: 2) Tighten 10 N·m (89 lb in)
6 | Front Fascia Tip Disconnect all electrical connectors.

## Front Bumper Fascia Replacement Solstice Turbo

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the brake cooling duct retainer. Refer to Front Brake Caliper Cooling Duct Replacement .

1 | Front Fascia Retainers (Qty: 5)
2 | Front Fascia Retainers (Qty: 6)
3 | Wheelhouse Liner Screws (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
4 | Front Fascia Bolts (Qty: 2) Tighten 10 N·m (89 lb in)
5 | Front Fascia Bolts (Qty: 4) Tighten 10 N·m (89 lb in)
6 | Front Fascia Tip Disconnect all electrical connectors.