For 1990-2009 cars

## Daytime Running Lamp Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Reposition either the left front or right front wheelhouse liner for access to the running lamp. Refer to Front Wheelhouse Liner Replacement .
3. Disconnect the fog lamp bulb socket electrical connector.
4. Disconnect the electrical connector harness for the DRL, Park and Turn Signal socket.

1 | Daytime Running, Park and Turn Signal Lamp Assembly Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Daytime Running, Park and Turn Signal Lamp Assembly

#### Procedure

1. Transfer the fog lamp assembly to the new DRL lamp assembly. Refer to Front Fog Lamp Replacement .
2. Aim the fog lamp after installation. Refer to Fog Lamp Aiming .