For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Disconnect the engine oil pressure sensor electrical connector (2).
3. Remove the engine oil pressure sensor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine oil pressure sensor and tighten to 22 N·m (16 lb ft).
2. Connect the engine oil pressure sensor electrical connector (2).
3. Lower the vehicle.