For 1990-2009 cars

## Instrument Panel Extension Trim Plate Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the instrument panel (I/P) cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the radio. Refer to Radio Replacement .
3. Remove the knee bolster panel. Refer to Knee Bolster Replacement .
4. Remove the I/P cup holder. Refer to Front Floor Console Cup Holder Replacement .

1 | Instrument Panel Extension Trim Plate Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Extension Trim Plate Assembly