For 1990-2009 cars

#### Special Tools

J 44765 Seal Installer

For equivalent regional tools, refer to Special Tools.

1. Inspect both inner and outer output shaft bearings for the following:

• | Damaged cage

• | Roller pitted

2. If either bearing is damaged replace extension housing.
3. Rotate the transmission 90 degrees.
4. Measure from the bottom to the face of the ouput shaft. Record this as dimension B. Refer to the End Play Specifications to determine the correct washer size.
5. Install the input and reaction carrier washer (22).
6. Install the input and reaction carrier thrust bearing (23) onto the extension housing.
7. Install the extension housing gasket (25) onto the extension housing (27).
8. Install the extension housing (27) onto the case.

Caution: Refer to Fastener Caution in the Preface section.

9. Install the extension housing bolts (35). Tighten the extension housing bolts to 22 N·m (16 lb ft).

Note: Install the seal onto the tool before installing into the case to prevent damage to the seal.

10. Using J 44765 seal installer install the prop shaft flange seal (29).