For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the interior trim panel. Refer to Door Trim Panel Replacement.

1 | Outside Door Handle Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Pull the upper corner of the water deflector down to access the outside handle bolts.
2. It is necessary to disengage the foam sound deadening block from inside the door to access the front door handle bolts. The bolt is hidden behind the foam block.
3. Release the lock rod from the lock cylinder and from the door latch.

Tighten
10 N·m (89 lb in)

2 | Front Door Outside Handle