For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement.
2. Program the audio amplifier after replacement. Refer to Control Module References.

1 | Radio Speaker Amplifier Bolt/Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Radio Speaker Amplifier Assembly