For 1990-2009 cars

## Driver Knee Bolster Bracket Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the knee bolster panel. Refer to Knee Bolster Replacement .

1 | Knee Bolster Bracket Bolt (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Knee Bolster Absorber
3 | Knee Bolster Bracket Assembly

## Driver Knee Bolster Bracket Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the knee bolster panel. Refer to Knee Bolster Replacement .

1 | Knee Bolster Bracket Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Driver Knee Bolster Bracket Assembly

#### Procedure

Remove the assembly line diagnostic link (ALDL) connector. Refer to Data Link Connector Replacement .