For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Front Bolts-to-Bracket | 49 N·m | 36 lb ft
A/C Compressor Rear Bolts-to-Bracket | 25 N·m | 19 lb ft
A/C Hi/Lo Pressure Switch | 5.5 N·m | 49 lb in
Air System Combination Valve Nuts | 7 N·m | 62 lb in
Air System Pipe-to-Exhaust Manifold Studs | 7 N·m | 62 lb in
Battery Hold Down Nut | 9 N·m | 80 lb in
Battery Negative Cable | 17 N·m | 13 lb ft
Battery Positive Cable | 17 N·m | 13 lb ft
Blower Motor Mounting Screws | 1.7 N·m | 15 lb in
Blower Unit Bracket-to-Cowl Bolt | 2.2 N·m | 20 lb in
Center Air Outlet Duct | 10 N·m | 89 lb in
Clutch Coil-to-Compressor Screws | 5 N·m | 44 lb in
Compressor Clutch Drive Plate-to-Compressor (Center Bolt) | 13 N·m | 9 lb ft
Compressor Pressure Relief Valve | 7.2 N·m | 63 lb in
Condenser Bracket-to-Radiator Bolts | 6 N·m | 60 lb in
Discharge Hose-to-Compressor | 25 N·m | 19 lb ft
Discharge Hose-to-Condenser Inlet | 23.5 N·m | 17 lb ft
Front Console Screws | 2.5 N·m | 20 lb in
Ground Wires-to-H-Brace | 2.2 N·m | 20 lb in
H-Brace-to-Front Floor Bracket | 25 N·m | 19 lb ft
HVAC Controller-to-I/P Retainer | 2.5 N·m | 22 lb in
HVAC Module-to-Beam Bolts | 6 N·m | 53 lb in
I/P Cluster Retaining Screws | 3 N·m | 27 lb in
I/P Endcap Retaining Screws | 2.5 N·m | 22 lb in
I/P Retainer Assembly Fasteners | 10 N·m | 89 lb in
I/P Upper Trim Panel Fastener | 6 N·m | 53 lb in
Inflator Module Bolts | 10 N·m | 89 lb in
Inflator Module Cover Fasteners | 2.2 N·m | 20 lb in
Liquid Line-to-Receiver Dehydrator | 14 N·m | 10 lb ft
Liquid Line-to-Thermal Expansion Valve | 25 N·m | 19 lb ft
Lower Heater Core Cover Screws | 1.7 N·m | 15 lb in
Lower Heater Duct | 1.7 N·m | 15 lb in
Radio Ground Strap-to-H-Brace | 2.2 N·m | 20 lb in
Radio-to-I/P Retainer | 2.5 N·m | 22 lb in
Rear Console Screws | 2.5 N·m | 22 lb in
Receiver-Dehydrator Hose-to-Condenser Outlet | 16.5 N·m | 12 lb ft
Receiver-Dehydrator Mounting Nut | 10 N·m | 89 lb in
Recirc Motor Mounting Screws | 1.7 N·m | 15 lb in
Seat Bolts | 35 N·m | 26 lb ft
Shifter Nuts | 25 N·m | 18 lb ft
Side Heater Core Cover Screws | 1.7 N·m | 15 lb in
Steering Column Bolts | 35 N·m | 26 lb ft
Steering Column Filler Panel Fasteners | 2.5 N·m | 22 lb in
Steering Column Shroud Fasteners | 1.5 N·m | 13 lb in
Suction Hose-to-Compressor | 25 N·m | 19 lb ft
Suction Hose-to-Thermal Expansion Valve | 25 N·m | 19 lb ft
Thermal Expansion Valve (TXV)-to-Evaporator | 10 N·m | 89 lb in
Windshield Defroster Nozzle | 2.2 N·m | 20 lb in