For 1990-2009 cars

# SATURN: REAR LICENSE PLATE RATTLES WHEN CLOSING REAR COMP

REVISION: 07/23/98 DIVS INVL 7 8

DUE TO THE ADDITION OF MODEL YEARS, THIS BULLETIN SUPERCEDES 98-T-04, WHICH SHOULD BE DISCARDED. ______________________________________________________________________

#### SUBJECT: REAR LICENSE PLATE RATTLES WHEN CLOSING REAR COMPARTMENT LID (INSTALL LICENSE PLATE BUMPER)

#### MODELS AFFECTED: 1996-1999 SATURN SEDANS AND 1997-1999 SATURN COUPES

#### CONDITION:

WHEN THE REAR COMPARTMENT LID IS CLOSED, THE REAR LICENSE PLATE MAY HIT AGAINST THE CENTER OF THE REAR COMPARTMENT LID LOWER OUTER PANEL, CAUSING A RATTLE.

#### CAUSE:

NO SUPPORT OR BUMPER FOR BOTTOM CENTER OF REAR LICENSE PLATE.

#### CORRECTION:

INSTALL ADDITIONAL REAR LICENSE PLATE BUMPER TO REAR COMPARTMENT LID LOWER OUTER PANEL ACCORDING TO THE PROCEDURE IN THIS BULLETIN.

#### PROCEDURE:

1. REMOVE REAR LICENSE PLATE FROM VEHICLE. . IF THE VEHICLE IS AN SL2 SEDAN, THE HOLE IS PRE-DRILLED AND NO DRILLING IS REQUIRED. PROCEED TO STEP 5 AND INSTALL REAR LICENSE PLATE BUMPER. . IF THE VEHICLE IS AN SL1 SEDAN, OR SC1 OR SC2 COUPE, DRILLING A NEW HOLE IS REQUIRED. PROCEED TO THE NEXT STEP.

2. MEASURE 130 MM (5 1/64 IN.) TOWARDS CENTER OF VEHICLE FROM EXISTING LEFT OR RIGHT REAR LICENSE PLATE BUMPER. THE HOLE SHOULD BE LEVEL WITH THE EXISTING HOLES USED FOR THE LEFT AND RIGHT REAR LICENSE PLATE BUMPER. (REFER TO ILLUSTRATION.) --------------------- FIGURE --------------------- 3. INSTALL A DRILL STOP 10 MM (25/64 IN.) ONTO EITHER A 5.5 MM OR 7/32 IN. DRILL, ALLOWING FOR A HOLE DEPTH OF 10 MM (25/64 IN). 4. DRILL HOLE IN REAR COMPARTMENT LID LOWER OUTER PANEL. 5. INSTALL REAR LICENSE PLATE BUMPER (P/N 21110594) INTO HOLE DRILLED INTO REAR COMPARTMENT LID LOWER OUTER PANEL. IF BUMPER FITS LOOSELY: A. REMOVE BUMPER AND APPLY KENT INDUSTRIES QUIK LEAK CHEK CLEAR SEALER (P/N 10510) (OR EQUIVALENT) TO BUMPER. B. INSTALL BUMPER AND REMOVE ANY EXCESS SEALER. 6. CLEAN AREA AND REPLACE LICENSE PLATE.

#### PARTS REQUIREMENTS:

21110594 BUMPER-RR LIC PLT 10510 KENT INDUSTRIES QUIK LEAK CHEK CLEAR SEALER

#### CLAIM INFORMATION:

TO RECEIVE CREDIT FOR THIS REPAIR DURING THE WARRANTY COVERAGE PERIOD, SUBMIT A CLAIM THROUGH THE SATURN DEALER SYSTEM AS FOLLOWS:

CASE TYPE DESCRIPTION LABOR OPERATION CODE TIME VW INSTALL LICENSE PLATE BUMPER T9777 0.2 HRR

FIGURES, 01

SATURN BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE YOUR SATURN RETAILER FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 SATURN CORPORATION U.S.A. ALL RIGHTS RESERVED.