For 1990-2009 cars

### Removal Procedure

Notice: When fasteners are removed, always reinstall them at the same location from which they were removed. If a fastener needs to be replaced, use the correct part number fastener for that application. If the correct part number fastener is not available, a fastener of equal size and strength (or stronger) may be used. Fasteners that are not reused, and those requiring thread-locking compound, will be called out. The correct torque values must be used when installing fasteners that require them. If the above procedures are not followed, parts or system damage could result.

1. Using a soft marker, mark around the striker for installation purposes.
2. Remove the screws.
3. Remove the striker and striker shim if present.

### Installation Procedure

1. Loosely install the striker and striker shim, if present, with screws.
2. Align the striker with the marks made prior to removal.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the screws.

Tighten
Tighten the rear door striker fasteners to 25 N·m (18 lb ft).

4. Check the door closing and align the striker as required.
5. Tighten the striker screws.