For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Terminal Bolts | 17 N·m | 13 lb ft
Cylinder Block Coolant Drain Plug | 35 N·m | 26 lb ft
Cylinder Block Drain Plugs | 35 N·m | 26 lb ft
Engine Mount-to-Front Cover Nuts | 50 N·m | 37 lb ft
Engine Mount-to-Midrail Bracket Nuts | 50 N·m | 37 lb ft
Fan Motor-to-Shroud Screws | 4 N·m | 35 lb in
Fan Nut | 3-5 N·m | 27-44 lb in
Lower Condenser Bracket-to-Radiator Bolts | 6 N·m | 53 lb in
Lower Transaxle Oil Cooler Line | 14 N·m | 10 lb ft
Midrail Bracket Bolts | 30 N·m | 22 lb ft
Radiator Support Brackets | 10 N·m | 89 lb in
Rubber Gasket | 5 N·m | 44 lb in
Surge Tank Attachment Bolts | 5 N·m | 44 lb in
Thermostat Housing-to-Block | 30 N·m | 22 lb ft
Upper Hold Down Bolt | 6 N·m | 53 lb in
Upper Radiator Hose and Clamp | 3.5 N·m | 31 lb in
Upper Transaxle Oil Cooler Line | 14 N·m | 10 lb ft
Washer Bottle Attachment Bolts | 4 N·m | 35 lb in
Water Pump Pulley-to-Water Pump Hub | 25 N·m | 19 lb ft
Water Pump-to-Block | 30 N·m | 22 lb ft
Wheel Nuts | 140 N·m | 103 lb ft