For 1990-2009 cars

### Waterleak Repair

To locate the exact leak point or to repair the leak, it may be necessary to remove some interior trim panels or components.

After completion of any waterleak repair, the general area should be retested using the waterstand test. Do not use an air hose or a water hose to test repaired areas. The repair material may dislodge under abnormal pressure application.