For 1990-2009 cars

## Seat Belt Retractor Replacement - Right Front Coupe

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the fasteners that attach the seat belt slide bar and remove slide bar.
3. Remove the seat belt retractor access door.
4. Remove the fastener and seat belt unit retractor.
5. Unsnap the seat belt bolt cover.
6. Loosen the captured fastener and rotate presenter arm forward to disengage the presenter arm guide notch from spaceframe.
7. After presenter arm is disengaged from spaceframe, completely loosen the captured fastener and remove the presenter arm assembly and the seat belt assembly.
8. Remove the presenter arm and the seat belt unit.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: Apply LOCTITE 242®, or equivalent, on all restraint fasteners prior to installation.

1. Install the presenter arm and the seat belt unit assembly.

Tighten
Tighten the presenter arm seat belt assembly - coupe to 50 N·m (37 lb ft).

2. Install the seat belt unit retractor and fastener.

Tighten
Tighten the seat belt unit retractor fastener to 50 N·m (37 lb ft).

3. Install the seat belt retractor access door.

Important: Make certain the cut and stitched side of the belt loop is facing outboard and the belt is straight as pictured.

4. Grasp the seat belt at the unattached end.
5. Rotate belt loop inboard to the center of vehicle 180 degrees rearward. Place loop over slide bar as shown.
6. Install the slide bar and fasteners.