For 1990-2009 cars

## Wiper Blade Element Replacement 1st Design

### Removal Procedure

Important: The right and left wiper blades are different lengths. Ensure that the longer blade is installed into the left-hand side.

Remove the existing wiper blade insert by pulling on the insert at the base of the wiper blade assembly until the insert is fully removed.

### Installation Procedure

Important: The wiper blade insert can be installed from either end of the wiper blade.

Important: Do not remove the retainer clips from the new wiper blade insert until installed.

1. Install the wiper blade insert by sliding it through the wiper blade claws until fully assembled into the wiper blade. Remove the clips as needed when sliding the insert through the claws.
2. Secure the wiper blade insert to the wiper blade by pulling the insert so that the notches engage into the heel claw.