For 1990-2009 cars

Table 1: | Design Specifications (SOHC L24/DOHC LL0)
Table 2: | Engine Block SOHC (L24)/DOHC (LL0)
Table 3: | Cylinder Head SOHC (L24)
Table 4: | Cylinder Head DOHC (LL0)
Table 5: | Engine Lubrication SOHC(L24)/DOHC (LL0)
Table 6: | Cam Drive System SOHC (L24)/DOHC (LL0)
Table 7: | Accessory Drive Belt/Tensioner SOHC (L24)/DOHC (LL0)
Table 8: | Cooling System SOHC (L24)/DOHC (LL0)

#### Design Specifications (SOHC L24/DOHC LL0)

Item | Specifications | Specifications
--- | --- | ---
Type - SOHC (L24) | Water Cooled - 4 Cycle SOHC |
Type - DOHC (LL0) | Water Cooled - 4 Cycle DOHC |
Horsepower - 1998 | SOHC (L24) - 100 hp at 5,000 RPM DOHC (LL0) - 124 hp at 5,600 RPM | SOHC (L24) - 74.5 Kw at 5,000 RPM DOHC (LL0) - 93 Kw at 5,600 RPM
Torque | SOHC (L24) - 114 lb ft at 2,400 RPM DOHC (LL0) - 122 lb ft at 4,800 RPM | SOHC (L24) - 155 N·m at 2,400 RPM DOHC (LL0) - 165N·m at 4,800 RPM
Cylinder Arrangement | 4 Cycle Inline, Transverse |
Bore and Stroke | 82 mm x 90 mm (3.2 in x 3.5 in) |
Compression Ratio | SOHC (L24) - 9.3:1 DOHC (LL0) - 9.5:1 |
Displacement | 1.9 liter (116 cu in) |
Valve Train - SOHC (L24) | 2 Valves Per Cylinder - SOHC |
Valve Train - DOHC (LL0) | 4 Valves Per Cylinder - DOHC |
Lubrication System | Pressure Feed |
Fuel System | Unleaded Grade Gasoline, 87 Octane (R+M) Divided by 2 |
Engine Net Weight (No Accessories) | SOHC (L24) DOHC (LL0) | 89.223 kg (196.74 lb) 99.872 kg (220.22 lb)

#### Engine Block SOHC (L24)/DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Cylinder Block
Top Side of Main Bearing Bore to Deck | 189.26 mm | 7.4511 in min | 189.26 mm | 7.4511 in min
Longitudinal Deck Warpage | 0.08 mm | 0.0031 in | 0.1 mm | 0.004 in max
Transverse Deck Warpage | 0.024 mm | 0.0009 in | 0.05 mm | 0.002 in max
Bore Diameter Middle |  |  |  |
(Bore No. 1, 2, 3) | 81.99-82.01 mm | 3.228-3.2287 in | 82.035 mm | 3.2297 in max
(Bore No. 4) | 82-82.02 mm | 3.2283-3.2291 in | 82.045 mm | 3.2301 in max
Re-boring Limit | -- | -- | 0.4 mm | 0.0157 in max
Bore Taper | 0.01 mm | 0.0004 in | 0.05 mm | 0.002 in max
Bore Out-of-Round | 0.01 mm | 0.004 in | 0.05 mm | 0.002 in max
Liner Height Depth | Flush | Flush | +/-0.013 mm | +/-0.005 in max
Piston
Piston Protrusion above Deck | 0.3 mm | 0.0118 in max | 0.379 mm | 0.0149 in max
Piston Protrusion below Deck | 0.066 mm | 0.0026 in max | 0.145 mm | 0.0057 in max
Skirt Outer Diameter, at 5 mm (0.2 in) from bottom of piston | 81.966-81.984 mm | 3.227-3.2277 in | 81.956 mm | 3.2266 in min
Piston-to-Ring (Top) | 0.04-0.08 mm | 0.0016-0.0032 in | 0.09 mm | 0.0035 in max
Piston-to-Ring (2nd) | 0.03-0.08 mm | 0.0012-0.0031 in | 0.08 mm | 0.0031 in max
Piston Pin Bore | 19.502-19.507 mm | 0.7678-0.768 in | 19.507 mm | 0.768 in max
Piston Pin Diameter | 19.496-19.5 mm | 0.7676-0.7677 in | 19.496 mm | 0.7676 in min
Piston Pin Clearance | 0.002-0.011 mm | 0.0001-0.0004 in | 0.011 mm | 0.0004 in max
Cylinder Clearance (Bore 1, 2, 3) | 0.006-0.044 mm | 0.0002-0.0017 in | 0.07 mm | 0.0028 in max
Cylinder Clearance (Bore 4) | 0.016-0.054 mm | 0.0006-0.0021 in | 0.07 mm | 0.0028 in max
Piston Ring
Ring End Gap (Top) | 0.25-0.4 mm | 0.0098-0.0157 in | 0.5 mm | 0.0197 in max
Ring End Gap (2nd) | 0.25-0.5 mm | 0.0098-0.0197 in | 0.6 mm | 0.0236 in max
Ring End Gap (Oil) | 0.25-1.25 mm | 0.0098-0.0492 in | 1.4 mm | 0.0551 in max
Connecting Rod
Piston Pin Bore to Crankshaft journal Bore | 144.97-145.03 mm | 5.707-5.709 in | 144.97 mm | 5.707 in min
Piston Pin Bushing Diameter | 19.506-19.520 mm | 0.7679-0.7685 in | 19.526 mm | 0.769 in max
Piston Pin-to-Rod Clearance | 0.006-0.024 mm | 0.0002-0.0009 in | 0.03 mm | 0.0012 in max
Large End Bore Diameter | 50.193-50.207 mm | 1.9761-1.9767 in | 50.207 mm | 1.9767 in max
Rod Journal Oil Clearance | 0.003-0.053 mm | 0.0001-0.0021 in | 0.063 mm | 0.0025 in max
Side Play on Crankshaft | 0.165-0.435 mm | 0.0065-0.01713 in | 0.47 mm | 0.0185 in max
Maximum Bend per 100 mm | 0.32 mm | 0.0126 in max | 0.32 mm | 0.0126 in max
Maximum Twist per 100 mm | 0.28 mm | 0.011 in max | 0.28 mm | 0.011 in max
Crankshaft
Main Journal Clearance | 0.006-0.05 mm | 0.0002-0.002 in | 0.06 mm | 0.0024 in max
Main Journal Diameter | 56.993-57.007 mm | 2.2438-2.2444 in | 56.99 mm | 2.2437 in min
Main Taper/Out-of-Round | 0.01 mm | 0.0004 in max | 0.01 mm | 0.0004 in max
Rod Pin Clearance | 0.01-0.065 mm | 0.00039-0.0025 in | 0.073 mm | 0.0029 in max
Rod Pin Diameter | 46.99-47.01 mm | 1.85-1.8508 in | 46.99 mm | 1.85 in min
Rod Tper/Out-of-Round (Rod Journal) | 0.012 mm | 0.0004 in max | 0.01 mm | 0.0004 in max
End Play | 0.05-0.2 mm | 0.002-0.0079 in | 0.25 mm | 0.0098 in max
Runout | 0.05 mm | 0.002 in max | 0.05 mm | 0.002 in max

#### Cylinder Head SOHC (L24)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Compression (Hot)
250 RPM (Open Throttle) | 1 310 kPa | 190 psi min | 1 241 kPa | 180 psi min
Cylinder Leakage (Hot)
689 kPa (100 psi) Input | 69 kPa (10% max) | 10 psi max | 138 kPa (15% max) | 20 psi max
Cylinder Head Warpage
Transverse Deck | 0.03 mm | 0.0012 in max | 0.05 mm | 0.002 in max
Longitudinal Deck | 0.07 mm | 0.0028 in max | 0.1 mm | 0.004 in max
Intake Flange (Overall) | 0.1 mm | 0.004 in max | 0.015 mm | 0.006 in max
Exhaust Flange (Overall) | 0.1 mm | 0.004 in max | 0.15 mm | 0.006 in max
Camshaft Bore (TIR) | 0.05 mm | 0.002 in max | 0.064 mm | 0.0025 in max
Cylinder Head
Lifter Bore Diameter (Intake and Exhaust) | 21.422-21.448 mm | 0.8434-0.8444 in | 21.45 mm | 0.8445 in max
Camshaft Bore Diameter | 44.475-44.5 mm | 1.751-1.752 in | 44.513 mm | 1.753 in max
Head Gasket Deck-to-Camshaft Cover Surface | 112.87-113.13 mm | 4.444-4.454 in |  |
Valve Guide Bore | 11.337-11.363 mm | 0.446-0.447 in | 11.368 mm | 0.448 in max
O.S. Guide Bore | 11.587-11.613 mm | 0.456-0.457 in | 11.613 mm | 0.457 in max
Intake Manifold
Head Flange Warpage | 0.13 mm | 0.005 in max | 0.2 mm | 0.008 in max
Throttle Body Flange Warpage | 0.1 mm | 0.004 in max | 0.15 mm | 0.006 in max
EGR Flange Warpage | 0.1 mm | 0.004 in max | 0.15 mm | 0.006 in max
Exhaust Manifold
Head Flange Warpage | 0.2 mm | 0.008 in max | 0.35 mm | 0.014 in max
Down Pipe Warpage | 0.4 mm | 0.016 in max | 0.4 mm | 0.016 in max
Camshaft
Thrust Clearance (End Play) | 0.07-0.2 mm | 0.0028-0.0079 in | 0.25 mm | 0.0098 in max
Journal Diameter | 44.399-44.424 mm | 1.748-1.749 in | 44.375 mm | 1.747 in min
Journal Oil Clearance | 0.051-0.101 mm | 0.002-0.004 in | 0.138 mm | 0.0054 in max
Camshaft Journal Runout (All) | 0.05 mm | 0.002 in max | 0.07 mm | 0.0028 in max
Camshaft Lobe Lift Rise (Intake and Exhaust) | 6.428-6.493 mm | 0.2531-0.2556 in | 6.4 mm | 0.252 in min
Lifter Body Diameter | 21.387-21.405 mm | 0.842-0.8427 in | 21.38 mm | 0.8417 in max
Lifter Body Oil Clearance | 0.017-0.061 mm | 0.0007-0.0024 in | 0.07 mm | 0.0028 in max
Lifter/Roller Total Length | 52.23-52.57 mm | 2.0563-2.0697 in | 52.15 mm | 2.0531 in min
Lifter Body Guide Flat | 19.18-19.3 mm | 0.7551-0.7598 in | 19.15 mm | 0.7539 in min
Lifter Guide Plate Width | 19.39-19.52 mm | 0.7634-0.7685 in | 19.385 mm | 0.7632 in max
Valve
Intake Stem Outer Diameter | 6.949-6.962 mm | 0.2736-0.2741 in | 6.935 mm | 0.273 in min
Exhaust Stem Outer Diameter | 6.931-6.95 mm | 0.2736-0.274 in | 6.915 mm | 0.272 in min
Valve Guide Inner Diameter | 6.987-7.013 mm | 0.2751-0.2761 in | 7.05 mm | 0.278 in max
Valve Guide Outer Diameter | 11.393-11.407 mm | 0.4485-0.4491 in |  |
Intake Stem to Guide Clearance | 0.025-0.064 mm | 0.001-0.0025 in | 0.115 mm | 0.004 in max
Exhaust Stem to Guide Clearance | 0.037-0.082 mm | 0.0015-0.0032 in | 0.135 mm | 0.005 in max
Intake Total Length | 138.53-139.05 mm | 5.45-5.47 in | 138.48-139.1 mm | 5.45-5.48 in
Exhaust Total Length | 138.73-139.25 mm | 5.46-5.48 in | 138.68-139.3 mm | 5.45-5.48 in
Intake Head Diameter | 39.87-40.13 mm | 1.5699-1.5799 in | -- | --
Exhaust Head Diameter | 33.87-34.13 mm | 1.3335-1.3437 in | -- | --
Intake Margin Width | 0.96-1.11 mm | 0.0378-0.0496 in | 0.9 mm | 0.035 in min
Exhaust Margin Width | 1.12-1.27 mm | 0.0441-0.0559 in | 1 mm | 0.039 in min
Face Angle (Intake and Exhaust) | 45-45.5° | 44.75-45.25° | 45-45.5° | 45-45.5°
Valve Tip Protrusion | 48.25-48.75 mm | 1.9-1.919 in | 48.8 mm | 1.921 in max
Valve Seat
Intake Width | 1-1.3 mm | 0.0394-0.0512 in | 1.6 mm | 0.063 in max
Exhaust Width | 1.3-1.6 mm | 0.0512-0.063 in | 1.9 mm | 0.075 in max
Angle (Intake and Exhaust) | 44.5-45.5° | 44.5-45.5° | 44.5-45° | 44.5-45°
Valve Set Outside Diameter |  |  |  |
Intake | 41.573-41.599 mm | 1.6377-1.638 in | -- | --
Exhaust | 35.073-35.099 mm | 1.381-1.382 in | -- | --
Seat Bore (Cylinder Head)
Intake | 41.487-41.513 mm | 1.633-1.634 in | -- | --
Exhaust | 34.987-35.013 mm | 1.377-1.378 in | -- | --
Valve Spring
Free Length (Intake and Exhaust) | 48.001-48.6 mm | 1.8898-1.9134 in | -- | --
Squareness | 2 mm | 0.08 in max | 2.5 mm | 0.1 in max
Force/Tension at 30 mm (1.18 in) | 898-983 N | 202-211 lbs | 870 N | 196 lbs min
Force/Tension at 41 mm (1.61 in) | 338-387 N | 76-87 lbs | 328 N | 75 lbs min
Rocker Arm
Shaft Diameter | 15.862-15.875 mm | 0.624-0.625 in | 15.86 mm | 0.62 in min
Spark Plug
Number | AC41-628 | --
Gap | 1 mm | 0.04 in | -- | --
Firing Order | 1-3-4-2 | --

#### Cylinder Head DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Compression (Hot)
250 RPM (Open Throttle) | 1 310 kPa | 190 psi min | 1 241 kPa | 180 psi min
Cylinder Leakage (Hot)
689 kPa (100 psi) Input | 69 kPa (10% max) | 10 psi max | 138 kPa (15% max) | 20 psi max
Cylinder Head Warpage
Transverse Deck | 0.03 mm | 0.0012 in max | 0.05 mm | 0.002 in max
Longitudinal Deck | 0.07 mm | 0.0028 in max | 0.1 mm | 0.004 in max
Intake Flange (Overall) | 0.1 mm | 0.004 in max | 0.015 mm | 0.006 in max
Exhaust Flange (Overall) | 0.1 mm | 0.004 in max | 0.15 mm | 0.006 in max
Camshaft Bore (TIR) | 0.05 mm | 0.002 in max | 0.064 mm | 0.0025 in max
Cylinder Head
Lifter Bore Diameter (Intake and Exhaust) | 33-33.025 mm | 1.2992-1.3002 in | 33.03 mm | 1.3 in max
Camshaft Bore Diameter | 29-29.026 mm | 1.141-1.142 in | 29.05 mm | 1.144 in max
Head Gasket Deck-to-Camshaft Cover Surface | 112.87-113.13 mm | 4.4449-4.4527 in | -- | --
Camshaft Cover-to-Plug Well Surface | 130.9-131.1 mm | 5.1535-51.614 in | -- | --
Valve Guide Bore | 11.337-11.363 mm | 0.446-0.447 in | 11.368 mm | 0.4475 in max
O.S. Guide Bore | 11.587-11.613 mm | 0.456-0.457 in | 11.613 mm | 0.457 in max
Valve Seat Bore
Intake | 33.399-33.423 mm | 1.315-1.316 in | -- | --
Exhaust | 28.399-28.423 mm | 1.118-1.119 in | -- | --
Intake Manifold
Head Flange Warpage | 0.13 mm | 0.0051 in max | 0.2 mm | 0.008 in max
Throttle Body Flange Warpage | 0.1 mm | 0.004 in max | 0.15 mm | 0.006 in max
EGR Flange Warpage | 0.1 mm | 0.004 in max | 0.15 mm | 0.006 in max
Exhaust Manifold
Head Flange Warpage | 0.25 mm | 0.01 in max | 0.35 mm | 0.014 in max
Down Pipe Warpage | 0.4 mm | 0.016 in max | 0.4 mm | 0.016 in max
Camshaft
Thrust Clearance (End Play) | 0.05-0.2 mm | 0.002-0.008 in | 0.25 mm | 0.01 in max
Journal Diameter | 28.95-28.97 mm | 1.1398-1.1406 in | 28.925 mm | 1.139 in min
Journal Oil Clearance | 0.03-0.076 mm | 0.0021-0.003 in | 0.125 mm | 0.005 in max
Camshaft Journal Runout (All) | 0.05 mm | 0.002 in max | 0.1 mm | 0.004 in max
Intake Cam Lobe Lift Rise | 8.96-9.04 mm | 0.3528-0.3599 in | 8.91 mm | 0.351 in min
Exhaust Cam Lobe Lift Rise | 8.66-8.74 mm | 0.3409-0.3441 mm | 8.61 mm | 0.339 in min
Lifter Body Diameter | 32.959-32.975 mm | 1.2976-1.2982 in | 32.947 mm | 1.297 in max
Lifter Body Oil Clearance | 0.017-0.061 mm | 0.0007-0.0024 in | 0.07 mm | 0.0028 in max
Lifter Body Clearance | 0.025-0.066 mm | 0.001-0.0026 in | 0.083 mm | 0.003 in max
Valve
Intake Stem Outer Diameter | 6.949-6.962 mm | 0.2736-0.274 in | 6.935 mm | 0.273 in min
Exhaust Stem Outer Diameter | 6.931-6.95 mm | 0.2726-0.2736 in | 6.919 mm | 0.272 in min
Valve Guide Inner Diameter | 6.987-7.013 mm | 0.275-0.276 in | 7.05 mm | 0.278 in max
Valve Guide Outer Diameter | 11.393-11.407 mm | 0.448-0.449 in |  |
Intake Stem to Guide Clearance | 0.025-0.064 mm | 0.001-0.0025 in | 0.113 mm | 0.004 in max
Exhaust Stem to Guide Clearance | 0.037-0.082 mm | 0.0015-0.0032 in | 0.131 mm | 0.005 in max
Intake Total Length | 100.72-101.18 mm | 3.9654-3.9835 in | 100.64-101.26 mm | 5.45-5.48 in
Exhaust Total Length | 100.02-101.48 mm | 3.9378-3.9559 in | 99.94-100.56 mm | 5.45-5.48 in
Intake Head Diameter | 32.16-32.46 mm | 1.2661-1.278 in | -- | --
Exhaust Head Diameter | 27.3-27.6 mm | 1.0748-1.0866 in | -- | --
Intake Margin Width |  |  | 0.75 mm | 0.035 in min
Exhaust Margin Width |  |  | 0.75 mm | 0.039 in min
Face Angle (Intake and Exhaust) | 45-45.5° | 45-45.5° | 45.5-45° | 45.5-45°
Valve Tip Protrusion | 40.95-41.55 mm | 1.612-1.636 in | 41.6 mm | 1.638 in max
Valve Seat
Intake Width | 0.79-1.23 mm | 0.0394-0.0512 in | 1.66 mm | 0.0653 in max
Exhaust Width | 1.05-1.49 mm | 0.0512-0.063 in | 1.92 mm | 0.0756 in max
Angle (Intake and Exhaust) | 44.5-45.5° | 44.5-45.5° | 44.5-45° | 44.5-45°
Valve Set Outside Diameter |  |  |  |
Intake | 33.49-33.51 mm | 1.3185-1.3193 in | -- | --
Exhaust | 28.49-28.5 mm | 1.121-1.122 in | -- | --
Valve Spring
Free Length (Intake and Exhaust) | 41.8 mm | 1.65 in | -- | --
Squareness | 2 mm | 0.08 in max | 2.5 mm | 0.1 in max
Force/Tension at 26.25 mm (0.984 in) | 724-788 N | 163-177 lbs | 688 N | 155 lbs min
Force/Tension at 35.25 mm (1.388 in) | 293-329 N | 66-74 lbs | 278 N | 63 lbs min
Spark Plug
Number | AC41-627 | --
Gap | 1 mm | 0.04 in | -- | --
Firing Order | 1-3-4-2 | --

#### Engine Lubrication SOHC(L24)/DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
SOHC (L24) Engine Oil Capacity:
Drain and Refill, No Filter Change | 3.4 L | 3.6 qt | -- | --
Drain and Refill, Filter Change | 3.8 L | 4 qt | -- | --
Dry Fill | 4.3 L | 4.5 qt | -- | --
DOHC (LL0) Engine Oil Capacity
Drain and Refill, No Filter Change | 3.4 L | 3.6 qt | -- | --
Drain and Refill, Filter Change | 3.8 L | 4 qt | -- | --
Dry Fill | 4.3 L | 4.5 qt | -- | --
Oil Pump
Displacement | 0.01267-0.01313 L/rev | 0.01339-0.01388 qt/rev 0.01112-0.01152 imp. qt/rev | -- | --
Tip Clearance | 0.15 mm | 0.006 in max | 0.15 mm | 0.006 in max
End-to-End Clearance | 0.04-0.125 mm | 0.0016-0.0049 in | 0.128 mm | 0.005 in max
Body-to-Side Clearance | 0.15-0.277 mm | 0.006-0.011 in | 0.277 mm | 0.011 in max
Regulator Valve
5W-30 EC II Oil (With Starburst Symbol) Pressure Setting at 90°C (195°F) Coolant Temperature at Idle RPM | 90 kPa | 13 psi min | 65 kPa | 9 psi min
at 2,000 RPM | 250 kPa | 36 psi min | 200 kPa | 29 psi min
Cold (Up to 2,500 RPM) | 560 kPa | 80 psi max | -- | --

#### Cam Drive System SOHC (L24)/DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Tensioner
Plunger Extended (Chain Installed, L24) | 1.5-10.5 mm | 0.059-0.413 in | 21 mm | 0.8626 in max
Plunger Extended (Chain Installed, LL0) | 1.5-9.5 mm | 0.059-0.374 in | 21 mm | 0.8626 in max
Chain
Length (Inner Diameter, L24) | 419-422 mm | 16.5-16.61 in | 425 mm | 16.73 in max
Length (Inner Diameter, LL0) | 581-584 mm | 22.87-22.99 in | 588 mm | 23.15 in max
Guide
Groove Wear (Chain Track) | 0 mm | 0 in | 2.5 mm | 0.0984 in max

#### Accessory Drive Belt/Tensioner SOHC (L24)/DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Belt/Pulley
Tension | 22.7-29.2 kg | 50-65 lbs | 20.4 kg | 45 lb min
Pulley Radial/Axial Runout | 0.38 mm | 0.015 in max | -- | --
Note: Measured at pulley belt grooves. |  |

#### Cooling System SOHC (L24)/DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Radiator
Capacity -SOHC (L24), Including Reservoir Tank | 6.75 L | 7 qt | -- | --
Capacity - DOHC (LL0), Including Reservoir Tank | 6.75 L | 7 qt | -- | --
Surge Tank Pressure Cap
Cap Opening Pressure | 89.6-138 kPa | 13-20 psi | -- | --
Vacuum Relief Setting | 0-6.9 kPa | 0-1 psi
Below Atmospheric Pressure
Torque | 2.5-3.5 N·m | 23-31 lb in |  |
Thermostat
Starts to Open | 84-88°C | 182-190°F | 83-89°C | 180-192°F
Full Open | 100°C | 212°F | 105°C | 222°F
Minimum Valve Lift at Full Open | 7.5 mm | 0.295 in | 6 mm | 0.236 in
Inlet Diameter | 38 mm | 1.4961 in | -- | --
Minimum Valve Leakage (Max. Pints After 5 Minutes) | 0.89 L max | 1.68 pts max | 0.94 L max | 2 pts max
Water Pump
Pulley Ratio (Crankshaft) | 1.3:1 |  | 1.3:1 |
Capacity at 6,000 RPM | 166.51/min | 176 qt/min | 151.41/min | 160 qt/min
| 146.1 imp qt/min |  | 132.8 imp qt/min
Inlet Housing Depth | 17.65-18.15 mm | 0.6949-0.7146 in | 17.648-18.152 mm | 0.6948-0.7146 in
Cooling Fan
Fan to Core Clearance | 25 mm | 0.9843 in | -- | --
Thermoswitch ON Temp | 105.5°C | 222°F | -- | --
Thermoswitch OFF Temp | 100.5°C | 213°F | -- | --
Antifreeze
| DEX-COOL™ | Mixture 50/50 |